;//------------------------------------------------------------------------------
;//  Copyright (C) 2008, Freescale Semiconductor, Inc. All Rights Reserved.
;//  THIS SOURCE CODE, AND ITS USE AND DISTRIBUTION, IS SUBJECT TO THE TERMS
;//  AND CONDITIONS OF THE APPLICABLE LICENSE AGREEMENT
;//
;//------------------------------------------------------------------------------


IF BSP_NOESDHC1!
IF BSP_ESDHC1
[HKEY_LOCAL_MACHINE\Drivers\BuiltIn\ESDHC1_MX25]
    "Order"=dword:21
    "Dll"="esdhc.dll"
    "Prefix"="SHC"
    "Index"=dword:1
    "DisableDMA"=dword:0                          ; Use this reg setting to disable internal DMA
    "MaximumClockFrequency"=dword:3197500         ; 52 MHz max clock speed
    ;"WakeupSource"=dword:1                                  ; this will enable system wakeup when card is inserted or removed during suspend state    

[HKEY_LOCAL_MACHINE\Comm\PegasSDN1\Parms]
    "SdioBitMode"=dword:00000001

[HKEY_LOCAL_MACHINE\Comm\PegasSDN1\Parms]
   "DisablePowerManagement"=dword:1
   "ResetOnResume"=dword:0
   "RebindOnResume"=dword:1
ENDIF ;BSP_ESDHC1  
ENDIF ;BSP_NOESDHC1!


IF BSP_NOESDHC2!
IF BSP_ESDHC2
[HKEY_LOCAL_MACHINE\Drivers\BuiltIn\ESDHC2_MX25]
    "Order"=dword:21
    "Dll"="esdhc.dll"
    "Prefix"="SHC"
    "Index"=dword:2
    "DisableDMA"=dword:0                          ; Use this reg setting to disable internal DMA
    "MaximumClockFrequency"=dword:3197500         ; 52 MHz max clock speed
    ;"WakeupSource"=dword:1 
ENDIF ;BSP_ESDHC2  
ENDIF ;BSP_NOESDHC2!

[HKEY_LOCAL_MACHINE\System\StorageManager\Profiles\MMC]
    "Name"="MMC Card"
    "Folder"="MMCMemory"

[HKEY_LOCAL_MACHINE\System\StorageManager\Profiles\SDMemory]
    "Name"="SD Memory Card"
    "Folder"="SDMemory"



