IF BSP_GPIO
[HKEY_LOCAL_MACHINE\Drivers\BuiltIn\GPIO]
   "Dll"="gpio.dll"         ; Driver DLL
   "Prefix"="GPI"           ; Driver name
   "Index"=dword:1	        ; Access the driver by opening "GPI1:"
   "Order"=dword:0	        ; No dependencies, start asap
   "Flags"=dword:8	        ; Naked flag (our function entry points do not start with the prefix. We use "Write", instead of "GPI_Write")
   
   ;Port 1 Safe GPIO Mask:
   ;31  28   24   20   16   12   8    4    0
   ; 1000 0000 0000 0000 0000 1000 0111 0000
   "Port1"=dword:80000870
   
   ;Port 2 Safe GPIO Mask:
   ;31  28   24   20   16   12   8    4    0
   ; 0000 0000 0011 0000 0000 1111 1111 1111
   "Port2"=dword:300FFF

   ;Port 3 Safe GPIO Mask:
   ;31  28   24   20   16   12   8    4    0
   ; 0000 0001 1010 1011 1100 0000 0000 0000
   "Port3"=dword:1ABC000

   ;Port 4 Safe GPIO Mask:
   ;31  28   24   20   16   12   8    4    0
   ; 0000 0000 0000 0000 0000 0001 1000 0000
   "Port4"=dword:180
 ENDIF
