IF BSP_LCD_AUTODETECT
[HKEY_LOCAL_MACHINE\Drivers\BuiltIn\LCDAD]
   "Dll"="LCDAD.dll"        ; Driver DLL
   "Prefix"="LAD"           ; Driver name
   "Index"=dword:1	        ; Access the driver by opening "LAD1:"
   "Order"=dword:1	        ; Make sure I2C driver is loaded
   "Flags"=dword:8	        ; Naked flag (our function entry points do not start with the prefix. We use "Write", instead of "LAD_Write")
 ENDIF
