;//------------------------------------------------------------------------------
;//  Copyright (C) 2009, Freescale Semiconductor, Inc. All Rights Reserved.
;//  THIS SOURCE CODE, AND ITS USE AND DISTRIBUTION, IS SUBJECT TO THE TERMS
;//  AND CONDITIONS OF THE APPLICABLE LICENSE AGREEMENT
;//
;//------------------------------------------------------------------------------

IF IMGNOKITL
IF BSP_FEC
[HKEY_LOCAL_MACHINE\Comm\FEC]
   "DisplayName"="FEC Ethernet Driver"
   "Group"="NDIS"
   "ImagePath"="fec.dll"

[HKEY_LOCAL_MACHINE\Comm\FEC\Linkage]
   "Route"=multi_sz:"FEC1"

[HKEY_LOCAL_MACHINE\Comm\FEC1]
   "DisplayName"="FEC Ethernet Driver"
   "Group"="NDIS"
   "ImagePath"="fec.dll"

[HKEY_LOCAL_MACHINE\Comm\FEC1\Parms]
   "BusNumber"=dword:0
   "BusType"=dword:0
   ; DuplexMode: 0:AutoDetect; 1:HalfDuplex; 2:FullDuplex.
   "DuplexMode"=dword:0
   ; The Ethernet Physical Address. For example,
   ; Ethernet Address 00:24:20:10:bf:03 is MACAddress1=0024,
   ; MACAddress2=2010,and MACAddress3=bf03.
   "MACAddress1"=dword:1213
   "MACAddress2"=dword:1728
   "MACAddress3"=dword:3120

[HKEY_LOCAL_MACHINE\Comm\FEC1\Parms\TcpIp]
   ; This should be MULTI_SZ
   "DefaultGateway"=""
   ; This should be SZ... If null it means use LAN, else WAN and Interface.
   "LLInterface"=""
   ; Use zero for broadcast address? (or 255.255.255.255)
   "UseZeroBroadcast"=dword:0
   ; Thus should be MULTI_SZ, the IP address list
   "IpAddress"="0.0.0.0"
   ; This should be MULTI_SZ, the subnet masks for the above IP addresses
   "Subnetmask"="0.0.0.0"
   "EnableDHCP"=dword:1

[HKEY_LOCAL_MACHINE\Comm\TcpIp\Parms]

   ;Set to True to keep the device from entering idle mode if there's network adapter 
    ;;"NoIdleIfAdapter"=dword:1
    ;Set to True to keep the device from entering idle mode while communicating/loop back 
    "NoIdleIfConnected"=dword:1


[HKEY_LOCAL_MACHINE\Comm\Tcpip\Linkage]
   ; This should be MULTI_SZ
   ; This is the list of llip drivers to load
   "Bind"=multi_sz:"FEC1"

ENDIF ;BSP_FEC
ENDIF ; IMGNOKITL