<?xml version="1.0" encoding="utf-8"?>
<CatalogFile xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:xsd="http://www.w3.org/2001/XMLSchema" RequiredVersion="6.00" xsi:schemaLocation="urn:Microsoft.PlatformBuilder/Catalog PbcXml600.xsd" xmlns="urn:Microsoft.PlatformBuilder/Catalog">
  <FileInformation Id="TopazBinary">
    <Title>TopazBinary</Title>
    <Description>Topaz BSP Catalog Items</Description>
    <Vendor>Device Solutions</Vendor>
    <OSVersion>6.00</OSVersion>
    <FileVersion>1.0.0.0</FileVersion>
  </FileInformation>
  <Bsp Id="TopazBinary">
    <Title>TopazBinary</Title>
    <Description>#DS:iMX25:DeviceSolutions:iMX25:ARMV5:Description</Description>
    <PlatformDirectory>TopazBinary</PlatformDirectory>
    <CpuId>Cpu:ARMV5</CpuId>
    <BspItemId>Item:Device Solutions:EthernetBootloader:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:KBDMOUSE_EVBKPD:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:I2CBUS1:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:I2CBUS2:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:I2CBUS3:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:BACKLIGHT LCD:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:LCD:im25-3ds_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:LCDAD:im25-3ds_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:ADC:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:TOUCH:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:UART1:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:UART2:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:UART3:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:UART4:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:UART5:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:High Speed OTG Port Full OTG Function:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:High Speed OTG Port Pure Client Function:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:High Speed OTG Port Pure Host Function:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:High Speed Host:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:USBFNMSC:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:USBFNSERIAL:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:USBFNRNDIS:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:DVFC:im25-3ds_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:CSPIBUS1:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:CSPIBUS2:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:CSPIBUS3:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:AUDIO:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:BATTERY:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:GPIO:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:GPT1:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:GPT2:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:GPT3:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:GPT4:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:FEC:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:PWRBTN:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:PWM1:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:PWM2:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:PWM3:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:PWM4:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:ESDHC1:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:ESDHC2:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:CANBUS1:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:CANBUS2:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:ESAI:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:SIM1:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:SIM2:imx25_Topaz</BspItemId>
    <BspItemId>Item:Device Solutions:NANDFMD:imx25_Topaz</BspItemId>
  </Bsp>
  <Item Id="Item:Device Solutions:EthernetBootloader:imx25_Topaz">
    <Title>#DS:iMX25:EthernetBootloader:Title</Title>
    <Description>#DS:iMX25:EthernetBootloader:Description</Description>
    <Type>BspSpecific</Type>
    <Location />
  </Item>
  <Item Id="Item:Device Solutions:KBDMOUSE_EVBKPD:imx25_Topaz">
    <Title>#DS:iMX25:KBDMOUSE_EVBKPD:Title</Title>
    <Description>#DS:iMX25:KBDMOUSE_EVBKPD:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_KEYPAD</Variable>
    <Module>KbdUs.dll</Module>
    <Location>Device Drivers\Input Devices</Location>
    <Notification>
      <Title>Default pin mux setup of the KEYPAD driver is mutually exclusive with the default pin mux setup of the UART3 and UART4 drivers!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:I2CBUS1:imx25_Topaz">
    <Title>#DS:iMX25:I2CBUS1:Title</Title>
    <Description>#DS:iMX25:I2CBUS1:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_I2CBUS1</Variable>
    <Module>i2c.dll</Module>
    <Location>Device Drivers\I2C Bus</Location>
  </Item>
  <Item Id="Item:Device Solutions:I2CBUS2:imx25_Topaz">
    <Title>#DS:iMX25:I2CBUS2:Title</Title>
    <Description>#DS:iMX25:I2CBUS2:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_I2CBUS2</Variable>
    <Module>i2c.dll</Module>
    <Location>Device Drivers\I2C Bus</Location>
    <Notification>
      <Title>Default pin mux setup of the I2C2 driver is mutually exclusive with the default pin mux setup of the CAN2 and PWM4 drivers!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:I2CBUS3:imx25_Topaz">
    <Title>#DS:iMX25:I2CBUS3:Title</Title>
    <Description>#DS:iMX25:I2CBUS3:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_I2CBUS3</Variable>
    <Module>i2c.dll</Module>
    <Location>Device Drivers\I2C Bus</Location>
    <Notification>
      <Title>Default pin mux setup of the I2C3 driver is mutually exclusive with the default pin mux setup of the CAN1, PWM2 and PWM3 drivers!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:BACKLIGHT LCD:imx25_Topaz">
    <Title>#DS:iMX25:BACKLIGHT LCD:Title</Title>
    <Description>#DS:iMX25:BACKLIGHT LCD:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_BACKLIGHT</Variable>
    <Module>lcdcbacklight.dll</Module>
    <Module>advbacklight.dll</Module>
    <Location>Device Drivers\Backlight</Location>
  </Item>
  <Item Id="Item:Device Solutions:LCD:im25-3ds_Topaz">
    <Title>#DS:iMX25:LCD:Title</Title>
    <Description>#DS:iMX25:LCD:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_LCD</Variable>
    <Module>lcdc.dll</Module>
    <Location>Device Drivers\Display</Location>
  </Item>
  <Item Id="Item:Device Solutions:LCDAD:im25-3ds_Topaz">
    <Title>#DS:iMX25:LCDAD:Title</Title>
    <Description>#DS:iMX25:LCDAD:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_LCD</Variable>
    <Variable>BSP_I2CBUS1</Variable>
    <Variable>BSP_LCD_AUTODETECT</Variable>
    <Module>lcdad.dll</Module>
    <Location>Device Drivers\Display</Location>
  </Item>
  <Item Id="Item:Device Solutions:UART1:imx25_Topaz">
    <Title>#DS:iMX25:UART1:Title</Title>
    <Description>#DS:iMX25:UART1:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_SERIAL_UART1</Variable>
    <Module>csp_serial.dll</Module>
    <Location>Device Drivers\Serial</Location>
    <Notification>
      <Title>Make sure UART1 is not selected as serial debug UART in the bootloader!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:UART2:imx25_Topaz">
    <Title>#DS:iMX25:UART2:Title</Title>
    <Description>#DS:iMX25:UART2:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_SERIAL_UART2</Variable>
    <Module>csp_serial.dll</Module>
    <Location>Device Drivers\Serial</Location>
    <Notification>
      <Title>Make sure UART2 is not selected as serial debug UART in the bootloader!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:UART3:imx25_Topaz">
    <Title>#DS:iMX25:UART3:Title</Title>
    <Description>#DS:iMX25:UART3:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_SERIAL_UART3</Variable>
    <Module>csp_serial.dll</Module>
    <Location>Device Drivers\Serial</Location>
    <Notification>
      <Title>Def pin mux setup of UART3 driver is mutually exclusive with default pin mux setup of KEYPAD driver! Do not select UART3 as debug UART in bootloader!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:UART4:imx25_Topaz">
    <Title>#DS:iMX25:UART4:Title</Title>
    <Description>#DS:iMX25:UART4:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_SERIAL_UART4</Variable>
    <Module>csp_serial.dll</Module>
    <Location>Device Drivers\Serial</Location>
    <Notification>
      <Title>Default pin mux setup of the UART4 driver is mutually exclusive with the default pin mux setup of the KEYPAD driver!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:UART5:imx25_Topaz">
    <Title>#DS:iMX25:UART5:Title</Title>
    <Description>#DS:iMX25:UART5:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_SERIAL_UART5</Variable>
    <Module>csp_serial.dll</Module>
    <Location>Device Drivers\Serial</Location>
    <Notification>
      <Title>Default pin mux setup of the UART5 driver is mutually exclusive with the default pin mux setup of the ESAI and SIM1 drivers!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:High Speed OTG Port Full OTG Function:imx25_Topaz">
    <Title>High Speed OTG Port Full OTG Function</Title>
    <Description>USB High Speed OTG Port Full OTG Function Driver</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_USB_HSOTG_CLIENT</Variable>
    <Variable>BSP_USB_HSOTG_HOST</Variable>
    <Variable>BSP_USB_HSOTG_XVC</Variable>
    <Module>imx_xvc.dll</Module>
    <ChooseOneGroup>true</ChooseOneGroup>
    <Location ConditionLocation="">Device Drivers\USB Devices\USB High Speed OTG Device</Location>
  </Item>
  <Item Id="Item:Device Solutions:High Speed OTG Port Pure Client Function:imx25_Topaz">
    <Title>High Speed OTG Port Pure Client Function</Title>
    <Description>USB High Speed OTG Port Pure Client Function Driver</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_USB_HSOTG_CLIENT</Variable>
    <Module>usbfn.dll</Module>
    <ChooseOneGroup>true</ChooseOneGroup>
    <Location>Device Drivers\USB Devices\USB High Speed OTG Device</Location>
  </Item>
  <Item Id="Item:Device Solutions:High Speed OTG Port Pure Host Function:imx25_Topaz">
    <Title>High Speed OTG Port Pure Host Function</Title>
    <Description>USB High Speed OTG Port Pure Host Function Driver</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_USB_HSOTG_HOST</Variable>
    <Module>hcd_hsotg.dll</Module>
    <ChooseOneGroup>true</ChooseOneGroup>
    <Location>Device Drivers\USB Devices\USB High Speed OTG Device</Location>
  </Item>
  <Item Id="Item:Device Solutions:High Speed Host:imx25_Topaz">
    <Title>USB Full Speed Host driver</Title>
    <Description>USB Full Speed Host Driver</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_USB_HSH2</Variable>
    <Module>hcd_hsh2.dll</Module>
    <Location>Device Drivers\USB Devices\USB Host Device</Location>
  </Item>
  <Item Id="Item:Device Solutions:USBFNMSC:imx25_Topaz">
    <Title>#DS:iMX25:USBFNMSC:Title</Title>
    <Description>#DS:iMX25:USBFNMSC:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_USBFN_MSC</Variable>
    <Variable>SYSGEN_USBFN_STORAGE</Variable>
    <ChooseOneGroup>true</ChooseOneGroup>
    <Location>Device Drivers\USB Devices\Default Function</Location>
  </Item>
  <Item Id="Item:Device Solutions:USBFNSERIAL:imx25_Topaz">
    <Title>#DS:iMX25:USBFNSERIAL:Title</Title>
    <Description>#DS:iMX25:USBFNSERIAL:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_USBFN_SERIAL</Variable>
    <Variable>SYSGEN_USBFN_SERIAL</Variable>
    <ChooseOneGroup>true</ChooseOneGroup>
    <Location>Device Drivers\USB Devices\Default Function</Location>
  </Item>
  <Item Id="Item:Device Solutions:USBFNRNDIS:imx25_Topaz">
    <Title>#DS:iMX25:USBFNRNDIS:Title</Title>
    <Description>#DS:iMX25:USBFNRNDIS:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_USBFN_RNDIS</Variable>
    <Variable>SYSGEN_USBFN_ETHERNET</Variable>
    <ChooseOneGroup>true</ChooseOneGroup>
    <Location>Device Drivers\USB Devices\Default Function</Location>
  </Item>
  <Item Id="Item:Device Solutions:ADC:imx25_Topaz">
    <Title>#DS:iMX25:ADC:Title</Title>
    <Description>#DS:iMX25:ADC:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_ADC</Variable>
    <Module>adc.dll</Module>
    <Location>Device Drivers\ADC</Location>
  </Item>
  <Item Id="Item:Device Solutions:TOUCH:imx25_Topaz">
    <Title>#DS:iMX25:TOUCH:Title</Title>
    <Description>#DS:iMX25:TOUCH:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_TOUCH</Variable>
    <Variable>BSP_ADC</Variable>
    <Module>touch.dll</Module>
    <Location>Device Drivers\Touch</Location>
  </Item>
  <Item Id="Item:Device Solutions:DVFC:im25-3ds_Topaz">
    <Title>#DS:iMX25:DVFC:Title</Title>
    <Description>#DS:iMX25:DVFC:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_DVFC</Variable>
    <Variable>BSP_I2CBUS1</Variable>
    <Module>dvfc_MC34704.dll</Module>
    <Location>Device Drivers\DVFC</Location>
  </Item>
  <Item Id="Item:Device Solutions:CSPIBUS1:imx25_Topaz">
    <Title>#DS:iMX25:CSPIBUS1:Title</Title>
    <Description>#DS:iMX25:CSPIBUS1:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_CSPIBUS1</Variable>
    <Module>cspi.dll</Module>
    <Location>Device Drivers\CSPI Bus</Location>
  </Item>
  <Item Id="Item:Device Solutions:CSPIBUS2:imx25_Topaz">
    <Title>#DS:iMX25:CSPIBUS2:Title</Title>
    <Description>#DS:iMX25:CSPIBUS2:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_CSPIBUS2</Variable>
    <Module>cspi.dll</Module>
    <Location>Device Drivers\CSPI Bus</Location>
    <Notification>
      <Title>Default pin mux setup of the CSPI2 driver is mutually exclusive with the default pin mux setup of the ESDHC1 driver!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:CSPIBUS3:imx25_Topaz">
    <Title>#DS:iMX25:CSPIBUS3:Title</Title>
    <Description>#DS:iMX25:CSPIBUS3:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_CSPIBUS3</Variable>
    <Module>cspi.dll</Module>
    <Location>Device Drivers\CSPI Bus</Location>
    <Notification>
      <Title>Default pin mux setup of the CSPI3 driver is mutually exclusive with the default pin mux setup of the ESAI, SIM1 and SIM2 drivers!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:AUDIO:imx25_Topaz">
    <Title>#DS:iMX25:AUDIO:Title</Title>
    <Description>#DS:iMX25:AUDIO:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_AUDIOSGTL</Variable>
    <Variable>BSP_I2CBUS1</Variable>
    <Module>wavedev2_sgtl5000.dll</Module>
    <Location>Device Drivers\Audio</Location>
  </Item>
  <Item Id="Item:Device Solutions:BATTERY:imx25_Topaz">
    <Title>#DS:iMX25:BATTERY:Title</Title>
    <Description>#DS:iMX25:BATTERY:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_BATTERY</Variable>
    <Module>battdrvr.dll</Module>
    <Location>Device Drivers\Battery</Location>
  </Item>
  <Item Id="Item:Device Solutions:GPIO:imx25_Topaz">
    <Title>#DS:iMX25:GPIO:Title</Title>
    <Description>#DS:iMX25:GPIO:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_GPIO</Variable>
    <Module>gpio.dll</Module>
    <Location>Device Drivers\GPIO</Location>
  </Item>
  <Item Id="Item:Device Solutions:GPT1:imx25_Topaz">
    <Title>#DS:iMX25:GPT1:Title</Title>
    <Description>#DS:iMX25:GPT1:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_GPT1</Variable>
    <Module>GPT.dll</Module>
    <Location>Device Drivers\GPT</Location>
  </Item>
  <Item Id="Item:Device Solutions:GPT2:imx25_Topaz">
    <Title>#DS:iMX25:GPT2:Title</Title>
    <Description>#DS:iMX25:GPT2:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_GPT2</Variable>
    <Module>GPT.dll</Module>
    <Location>Device Drivers\GPT</Location>
  </Item>
  <Item Id="Item:Device Solutions:GPT3:imx25_Topaz">
    <Title>#DS:iMX25:GPT3:Title</Title>
    <Description>#DS:iMX25:GPT3:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_GPT3</Variable>
    <Module>GPT.dll</Module>
    <Location>Device Drivers\GPT</Location>
  </Item>
  <Item Id="Item:Device Solutions:GPT4:imx25_Topaz">
    <Title>#DS:iMX25:GPT4:Title</Title>
    <Description>#DS:iMX25:GPT4:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_GPT4</Variable>
    <Module>GPT.dll</Module>
    <Location>Device Drivers\GPT</Location>
  </Item>
  <Item Id="Item:Device Solutions:FEC:imx25_Topaz">
    <Title>#DS:iMX25:FEC:Title</Title>
    <Description>#DS:iMX25:FEC:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_FEC</Variable>
    <Module>FEC.dll</Module>
    <Location>Device Drivers\FEC</Location>
    <Notification>
      <Title>Default pin mux setup of the FEC driver is mutually exclusive with the default pin mux setup of the ESDHC2 driver!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:PWRBTN:imx25_Topaz">
    <Title>#DS:iMX25:PWRBTN:Title</Title>
    <Description>#DS:iMX25:PWRBTN:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_PWRBTN</Variable>
    <Module>pwrbtn.dll</Module>
    <Location>Device Drivers\Power Button</Location>
  </Item>
  <Item Id="Item:Device Solutions:PWM1:imx25_Topaz">
    <Title>#DS:iMX25:PWM1:Title</Title>
    <Description>#DS:iMX25:PWM1:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_PWM1</Variable>
    <Module>pwm.dll</Module>
    <Location>Device Drivers\PWM</Location>
  </Item>
  <Item Id="Item:Device Solutions:PWM2:imx25_Topaz">
    <Title>#DS:iMX25:PWM2:Title</Title>
    <Description>#DS:iMX25:PWM2:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_PWM2</Variable>
    <Module>pwm.dll</Module>
    <Location>Device Drivers\PWM</Location>
    <Notification>
      <Title>Default pin mux setup of the PWM2 driver is mutually exclusive with the default pin mux setup of the CAN1 and I2C3 drivers!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:PWM3:imx25_Topaz">
    <Title>#DS:iMX25:PWM3:Title</Title>
    <Description>#DS:iMX25:PWM3:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_PWM3</Variable>
    <Module>pwm.dll</Module>
    <Location>Device Drivers\PWM</Location>
    <Notification>
      <Title>Default pin mux setup of the PWM3 driver is mutually exclusive with the default pin mux setup of the CAN1 and I2C3 drivers!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:PWM4:imx25_Topaz">
    <Title>#DS:iMX25:PWM4:Title</Title>
    <Description>#DS:iMX25:PWM4:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_PWM4</Variable>
    <Module>pwm.dll</Module>
    <Location>Device Drivers\PWM</Location>
    <Notification>
      <Title>Default pin mux setup of the PWM4 driver is mutually exclusive with the default pin mux setup of the CAN2 and I2C2 drivers!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:ESDHC1:imx25_Topaz">
    <Title>#DS:iMX25:ESDHC1:Title</Title>
    <Description>#DS:iMX25:ESDHC1:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_ESDHC1</Variable>
    <Module>esdhc.dll</Module>
    <Location>Device Drivers\SD Controller</Location>
  </Item>
  <Item Id="Item:Device Solutions:ESDHC2:imx25_Topaz">
    <Title>#DS:iMX25:ESDHC2:Title</Title>
    <Description>#DS:iMX25:ESDHC2:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_ESDHC2</Variable>
    <Module>esdhc.dll</Module>
    <Location>Device Drivers\SD Controller</Location>
    <Notification>
      <Title>Default pin mux setup of the ESDHC2 driver is mutually exclusive with the default pin mux setup of the FEC driver!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:CANBUS1:imx25_Topaz">
    <Title>#DS:iMX25:CANBUS1:Title</Title>
    <Description>#DS:iMX25:CANBUS1:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_CANBUS1</Variable>
    <Module>can.dll</Module>
    <Location>Device Drivers\CAN Bus</Location>
    <Notification>
      <Title>Default pin mux setup of the CAN1 driver is mutually exclusive with the default pin mux setup of the I2C3, PWM2 and PWM3 drivers!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:CANBUS2:imx25_Topaz">
    <Title>#DS:iMX25:CANBUS2:Title</Title>
    <Description>#DS:iMX25:CANBUS2:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_CANBUS2</Variable>
    <Module>can.dll</Module>
    <Location>Device Drivers\CAN Bus</Location>
    <Notification>
      <Title>Default pin mux setup of the CAN2 driver is mutually exclusive with the default pin mux setup of the PWM4 driver!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:ESAI:imx25_Topaz">
    <Title>#DS:iMX25:ESAI:Title</Title>
    <Description>#DS:iMX25:ESAI:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_ESAI</Variable>
    <Variable>BSP_CSPIBUS1</Variable>
    <Variable>BSP_I2CBUS1</Variable>
    <Module>esai_wm8580.dll</Module>
    <Location>Device Drivers\ESAI</Location>
    <Notification>
      <Title>Default pin mux setup of the ESAI driver is mutually exclusive with the default pin mux setup of the SIM1 and UART5 drivers!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:SIM1:imx25_Topaz">
    <Title>#DS:iMX25:SIM1:Title</Title>
    <Description>#DS:iMX25:SIM1:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_SMARTCARD_SIM1</Variable>
    <Module>sim.dll</Module>
    <Location>Device Drivers\SIM</Location>
    <Notification>
      <Title>Default pin mux setup of the SIM1 driver is mutually exclusive with the default pin mux setup of the ESAI and UART5 drivers!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:SIM2:imx25_Topaz">
    <Title>#DS:iMX25:SIM2:Title</Title>
    <Description>#DS:iMX25:SIM2:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_SMARTCARD_SIM2</Variable>
    <Module>sim.dll</Module>
    <Location>Device Drivers\SIM</Location>
    <Notification>
      <Title>Default pin mux setup of the SIM2 driver is mutually exclusive with the default pin mux setup of the ESAI driver!</Title>
      <Html />
    </Notification>
  </Item>
  <Item Id="Item:Device Solutions:NANDFMD:imx25_Topaz">
    <Title>#DS:iMX25:NANDFMD:Title</Title>
    <Description>#DS:iMX25:NANDFMD:Description</Description>
    <Type>BspSpecific</Type>
    <Variable>BSP_NANDFMD</Variable>
    <Module>flashpdd_nand.dll</Module>
    <Location>Device Drivers\NAND</Location>
  </Item>
</CatalogFile>