;//------------------------------------------------------------------------------
;//  Copyright (C) 2008, Freescale Semiconductor, Inc. All Rights Reserved.
;//  THIS SOURCE CODE, AND ITS USE AND DISTRIBUTION, IS SUBJECT TO THE TERMS
;//  AND CONDITIONS OF THE APPLICABLE LICENSE AGREEMENT
;//
;//------------------------------------------------------------------------------

[HKEY_CURRENT_USER\ControlPanel\Backlight]
    "BattBacklightLevel"=dword:7F  ; Backlight level settings. 0xFF = Full On
    "ACBacklightLevel"=dword:7F    ; Backlight level settings. 0xFF = Full On

    "ACTimeout"=dword:3c            ; On AC power turn backlight off after 60 seconds
    "UseExt"=dword:1                ; Enable turning off backlight when on AC power
    "BatteryTimeout"=dword:1e       ; On battery power turn backlight off after 30 seconds
    "UseBattery"=dword:1            ; Enable turning off backlight when on battery power
    "AdvancedCPL"="AdvBacklight"    ; Enable Advanced Backlight control panel dialog
    
; HIVE BOOT SECTION
; Turn off backlight in SystemIdle
[HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Control\Power\State\SystemIdle]
    "bkl1:"=dword:4                 ; Backlight off in SystemIdle (synchronize with LCD) NOTE: device name needs to be lower case!
    
; END HIVE BOOT SECTION
    