;
; Copyright (c) Microsoft Corporation.  All rights reserved.
;
;
; Use of this source code is subject to the terms of the Microsoft end-user
; license agreement (EULA) under which you licensed this SOFTWARE PRODUCT.
; If you did not accept the terms of the EULA, you are not authorized to use
; this source code. For a copy of the EULA, please see the LICENSE.RTF on your
; install media.
;
;------------------------------------------------------------------------------
;
; Copyright (C) 2004-2009, Freescale Semiconductor, Inc. All Rights Reserved.
; THIS SOURCE CODE, AND ITS USE AND DISTRIBUTION, IS SUBJECT TO THE TERMS
; AND CONDITIONS OF THE APPLICABLE LICENSE AGREEMENT 
;
;------------------------------------------------------------------------------
;
;         OS MEMORY MAP                       BOOTLOADER MEMORY MAP
;
;                       +---- 8000.0000 ----+
;           ARGS (4 KB) |                   | ARGS (4 KB)
;                       +---- 8000.1000 ----+
;       CSPDDK (32 KB)  |                   |
;                       +---- 8000.9000     | XLDR Image / Bootloader Stack (236 KB)
;                       |                   |
;                       |     8003.C000 ----+
;                       |                   | Bootloader Page Table (16 KB)
;                       |     8004.0000 ----+
;                       |                   | Bootloader Image (256 KB)
;                       |     8008.0000 ----+
;                       |                   | Bootloader RAM (256 KB)
;                       +---- 800C.0000 ----+
; USB KITL DMA (240 KB) |                   | USB KITL DMA (240 KB)
;                       +---- 800F.C000 ----+
;       FEC DMA (16 KB) |                   | FEC DMA (16 KB) 
;                       +---- 8010.0000 ----+
;                       |                   |
;                       |                   |
;      NK Image (16 MB) |                   |
;                       |                   |
;                       |                   |
;        **auto-size**  +---- 8110.0000     | Flash Cache
;                       |                   | 
;                       |                   |
;                       |                   |
;       NK RAM (47 MB)  |                   |
;                       |                   |
;                       |                   |
;                       |                   |
;                       +---- 8400.0000 ----+
;
;------------------------------------------------------------------------------

;**************************** MEMORY SECTION ***************************
MEMORY

; --------------------------- RAM image --------------------------------
;   Start Addr      End Addr        Mem Type    Region Name     Size
;   0x80000000      0x80100000      SDRAM       reserved         1 MB
;   0x80100000      0x81100000      SDRAM       NK              16 MB
;   0x81100000      0x84000000      SDRAM       RAM             47 MB
; ----------------------------------------------------------------------
;                   Name            Address     Size        Type
                    BOOT_AND_OTHER  80000000    00100000    RESERVED
                    NK              80100000    01000000    RAMIMAGE
                    RAM             81100000    02F00000    RAM

;**************************** CONFIG SECTION ***************************
CONFIG

; ---------------------- All Image Types Settings ----------------------
;   KERNELFIXUPS = ON (sections to which the kernel can write are 
;                      relocated to the start of RAM)
;   SRE = ON (Romimage.exe produces an .sre file)
; ----------------------------------------------------------------------
    KERNELFIXUPS=ON

; --------------------------- RAM image --------------------------------
;   AUTOSIZE = ON (allows NK and RAM space to resize automatically)
;   ROMSIZE  = 0x02000000 (32 MB)
;   ROMSTART = 0x80100000 (NK virtual address base)
;   ROMWIDTH = 32 (32-bit wide memory, entire image in one file)
; ----------------------------------------------------------------------

AUTOSIZE=ON
ROMSIZE= 02000000
ROMSTART=80100000
ROMWIDTH=32
    
IF IMGFLASH
    
    IF IMGSDMMC
        ; ROMOFFSET = (SD/MMC LOGICAL ADDRESS - NK START ADDRESS) % 0x100000000
        ;           = ( 0x93700000 + 0x00080000  -  0x80100000     ) % 0x100000000 = 
        ROMOFFSET=13680000
    ELSE
		; NAND Flash Memory
		; ROMOFFSET = (FLASH LOGICAL ADDRESS - NK START ADDRESS) % 0x100000000
        ;           = ( 0x91300000 + 0x00280000  -  0x80100000     ) % 0x100000000 = 
        ROMOFFSET=11480000
	ENDIF
    
ENDIF

; ------------------------------ COMPRESSION ---------------------------
;   NK COMPRESSION
; ----------------------------------------------------------------------
; @CESYSGEN IF !NK_NKNOCOMP
    COMPRESSION=ON
; @CESYSGEN ENDIF !NK_NKNOCOMP
; @CESYSGEN IF NK_NKNOCOMP
    COMPRESSION=OFF
; @CESYSGEN ENDIF NK_NKNOCOMP

; ---------------------- Profiling-enabled kernel ----------------------
;   PROFILE = ON (includes profiler structure and symbols in image)
; ----------------------------------------------------------------------
IF IMGPROFILER
   PROFILE=ON
ENDIF

; --------------------- Profiling-disabled kernel ----------------------
;   PROFILE = OFF (does not include profiler structure and symbols)
; ----------------------------------------------------------------------
IF IMGPROFILER !
   PROFILE=OFF
ENDIF

;
; ROMFLAGS is a bitmask of options for the kernel
;   ROMFLAGS    0x0001  Disallow Paging
;   ROMFLAGS    0x0002  Not all KMode
;   ROMFLAGS    0x0010  Trust Module only
;
IF IMGTRUSTROMONLY
    IF IMGNOTALLKMODE
       ROMFLAGS=12
    ENDIF
    IF IMGNOTALLKMODE !
       ROMFLAGS=10
    ENDIF
ENDIF

IF IMGTRUSTROMONLY !
    IF IMGNOTALLKMODE
       ROMFLAGS=2
    ENDIF
    IF IMGNOTALLKMODE !
       ROMFLAGS=0
    ENDIF
ENDIF

; FSRAMPERCENT is used to select the percentage of the RAM dedicated to the file system
; check http://msdn.microsoft.com/en-us/library/aa908688.aspx for more info.
; FSRAMPERCENT=0x20202020 => 12.5 % of RAM is used for the file system
FSRAMPERCENT=0x20202020 

; EOF config.bib
